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[bookmark: _pbbvj2cqb2up]SMM 7.2.5 Lockout/Tagout Checklist
Definition:
Lockout/Tagout: working on electrical power systems aboard UW MAROPS vessels. 

Checklist:
· All personnel have been informed of the pending operation and affected equipment  secured to avoid damaging essential components.  
· The Lock Out/Tag Out Record has been posted.
· Your supervisor has ensured that the proper protective equipment for the assigned task is supplied and in use.
· A separate sign has been posted in the space warning everyone that electrical work is in progress and marked circuits are secured for safety.
· The Chief Engineer has identified all potential circuits, valves, and systems which may be impacted by an assigned task.    
· Multiple power sources have been identified and secured. (e.g. UPS, propulsion motor    heaters, etc.)
· Identified circuits at all controlling locations are tagged with a red tag and all power sources to that circuit secured.
· The controlling locations, circuits, valves, and systems have been secured by a lock and key.  The key has been identified by a red tag noting the circuit number. 
· The key and tag have been posted in the Engine Control Room on the Safety Bulletin board.  
· Conduct a briefing between those involved with the work including any vendors/contractors. 
· After the work is completed and tested, the lock and tags have been removed and notices taken down from the Safety bulletin boards.

Record Sheet:
The following equipment/system has been (circle one):	Locked Out		Tagged Out
Date/Time:____________________________________________________________________
Equipment/System:_____________________________________________________________
Circuit(s), Valve(s), System(s):____________________________________________________
_____________________________________________________________________________
By Who:______________________________________________________________________
Why:_________________________________________________________________________
Lock/Tag:_____________________________________________________________________
Authorized by Chief Engineer or designee:___________________________________________

Work Completed Checklist:
· After work is completed, the LOTO has been removed, and all circuits/systems have been restored to normal condition
· All personnel who were impacted by this LOTO have been informed that the task is complete

Lock Out/Tag Out Release:
Date/Time:____________________________________________________________________
By Who:______________________________________________________________________
Equipment/System Test & Restore:_________________________________________________
Authorized by Chief Engineer or designee:___________________________________________
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